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Abstract: The authors have witnessed and been part of the development of the burgeoning complexities of weapons systems. They have focused some of their research on the need to analyze the life-cycle sustainment of these systems.  This sustainment analysis has similarly grown in complexity and sophistication.  To be optimally useful, the results and insights from these analyses need to be accessible long before the systems are fielded and before sustainment parameters can be established and sustainment data collected from live implementations.  This strongly supports the need to employ both constructive and virtual simulations to provide pre-deployment “experience” with systems. These simulations must be programmed to include the various input and output parameters of the system-engineered sustainment model. The size of modern weapons systems and the wide geographical dispersion of such systems calls for significant computational capabilities; this need is exacerbated by the current focus on simulating operations in large urban areas, fully populated by red, blue and civilian populations, all suitably programmed to act in a demographically appropriate way. Because a major factor of sustainment is maintenance and that maintenance is dramatically impacted by environmental factors, the modeling of these factors, along with verifiable functions representing their impact on hardware and personnel, must be modeled as well.  There is a long history of using high performance computing to enable and enhance large-scale simulations and some of the authors have been part of that development process since 1995. Further, new advances in computing now offer to create a new computational paradigm for high performance computing, e.g. the innovations at the University of Southern California, Quantum Computing Center.  As Systems Engineering has co-evolved with these computational advances, it has made good use of Markov and martingale analyses, and one of the authors is currently developing a model that relies on this sub-discipline of analysis to better characterize the sustainment of weapons systems. Serendipitously, this line of inquiry is well situated to make excellent use of the quantum annealer at USC, as Markov processes are the foundation of the annealer’s operations,   This paper will briefly describe the need for and the current state of the art of sustainment analyses, lay out the need for improved and expanded simulation techniques, and discuss the path to facilitating the implementation these across the entire spectrum of the simulation community. Alternative approaches, interoperability challenges, and future developments will be suggested, outlined and documented.

  
[bookmark: 1._This_is_a_Section_Title_[“Heading_1”_]Introduction

There is a broadening of the capabilities of simulation for the DoD.  Advanced technologies and more sophisticated analytical techniques are expanding the scope of the dual simulation trilogies of modality: Live, Virtual and Constructive and utilization: Training, Evaluation and Analysis. The DoD Acquisition community asserts that “the goal is to ensure sustainment considerations are integrated into all … activities”. [0] This paper will focus on the needs and possible contributions of the Systems Engineering community, the impact of the parameterization of life-cycle analyses using Markov, Hidden Markov and martingale analyses, and the contributions of the High Performance Computing discipline, most particularly, the emergence of quantum computing as an emerging technology.  The underlying issues to be addressed are : “What can the sustainment professionals contribute to the Simulation community to improve their product?” and “What can the Simulation community contribute to the Sustainment professionals to optimize their analyses.” On-going research and early insights will be reported as they are made available.  


[bookmark: 1.1_This_is_a_subsection_title_[“Heading]Background

Since the earliest days of warfare, leaders have sought to understand and prepare for combat through simulations of one kind or another.  Early athletics often evolved as competitive test of combat skills in a non-combat arena [1]. Many games such as chess were centered on abstracting and emulating combat [2].  More complex and realistic simulations evolved over the centuries, but they all had in common trying to train people to behave well in combat, trying to see if some new weapon would be effective, or trying to better predict the outcome of an impending operation [3].  Within the professional experience of the authors, simulations have expanded their capabilities along several axes, including: geographical area, resolution of simulated objects, richness of behaviors, duration of simulations, speed of performance (e.g. computer generated constructive simulations can be run at significantly faster than real time), and sophistication of analytic tools to better understand the large amounts of data collected [4]. Many of these advances have been enabled by the use of High Performance Computing (HPC) [5]


[bookmark: 2._Reminder]Current Practice

It has been the authors’ experience that battlefield simulations rarely take heedexperience that Major Acquisition Programs, Life Cycle support and battlefield simulations rarely take heed of system degradation over time and they can think of no occasion when the Systems Engineering parameters surrounding life-cycle sustainment were incorporated into the functions of the simulation code.  This impacts all three of the simulation modalities and all three of the uses of simulation in two ways: it makes the simulations less valid and it deprives the Program Managers Systems Engineers of valuable insights into life-cycle sustainment issues. 



[bookmark: 3._References]New Approach

Half a page describing how we can marshal capabilities to meet otherwise daunting challenges. 

In 1982 Senator Sam Nunn and Congressman David McCurdy passed legislation that became permanent in 1983 for Department of Defense Weapons Procurement programs. The legislation requires notification to congress if unit cost goes above 25% and program termination if costs rise above 50%. There are provisions where the Secretary of Defense (SECDEF can certified: the program is essential to national security, that no suitable alternative of lesser cost is available; new estimates of total program costs are reasonable; and management structure is (or has been made) adequate to control costs.  

In the authors opinion that as Sustainment options fall into the latter part of the Life Cycle Sustainment IAW with Chart 1 (Insert Chart 1),   

[image: ]

[image: ]


 it remains ripe for budget cutting measures as costs rise in the earlier part of the life cycle.  High performance computing in the for of Quantum Annealers and Parameterization is a new approach that illuminates way for SE’s to keep costs on track and below Nunn McCurdy breech thresholds. SE’s will then have new trigger point capabilities to alert the PM’s that their acquisition program is in heading toward the breech thresholds that are not capable under current modeling and simulation approaches. Quantum Annealers will give PM’s the ability to not only avoid Breech but by maintaining real cost savings larger acquisition quantities can be realized.  


SEystems engineering and Simulation 

Modeling and Simulation (M&S) can effectively be employed in support of SE.  It is extremely costly to design, build and test hardware and then find out after the test program, that the desired system does not meet the requirements or quite possibly does not function as intended.  Effective and validated M&S can significantly reduce the cost of the Design-Build-Test Repeat until right scenario.  A accurate model, such as a physics based model where ultimately the model is the specification, can be affordably developed and exercised to produce data which then will be analyzed to determine if the system can meet the defined requirements. If not, then modifications can quickly be made to the model and then iterated until the desired outcome is obtained.  With that said, a model that is not validated, poses significant risk when employing that model to design a component, system, or experiment.  It is always necessary to compare data obtained from M&S with data that is empirically derived even at subscale.  If the data resulting from the model reasonably agrees with that obtained empirically, then the only challenge that needs to be addressed is scalability and that is why developing a physics based model is important, as the risk of scalability is mitigated through the use of models based on physics. A key tenant of SE is the identification, reduction and mitigation of risk.  Cost is a defined risk factor.  The application of validated M&S tools will reduce the risk of cost overrun in the design, development, testing, certifying and employing complex systems.  One paragraph to half a page on SE 

1.1.1 Requirements

One or two paragraphs on what SE needs from simulations  As stated in the previous paragraph, simulations produce data.  That data then has to be analyzed and assessed to determine if the system will meet the specified requirements.  The SE process will use the results of that analysis and inform decisions (i.e. data driven decisions) that need to be made with respect to any modifications that need to be made to the model to produce the desired result.  It is this iterative process, employing the model and results of the model, through 1) Requirements, 2) Functional Analysis, and 3) Synthesis until the desired outcome is obtain.  In essence, SE needs validated data resulting from M&S to make informed decisions and thereby reduce and mitigate risk.


1.1.2 Contributions

One or two paragraphs on how S#E can make sims better The SE process can improve simulations through the discipline of iteration of the model until the desired outcome is obtained.  The validity of simulations is determined by 1) the accuracy of the assumptions that go into the model or simulation and 2) how closely the model and its formulations accurately represents the real world, and in this case, the physical system that it is representing.  The three ingredients of SE include: 1) Requirements, 2) Functional Analysis and 3) Synthesis.  The outcome of simulation is manifested in the third ingredient, Synthesis.  However, the process by which the model reaches this point is through the first two ingredients, Requirements and Functional Analysis.  First and foremost, the requirement needs to be established, and serves as the foundation for the model or simulation.  This requirement also serves as a given or assumption for the model.  If the requirement is inaccurate, then the model will be right for the requirement, but will be wrong for the system that the model represents.  The requirement must be correct initially, and if not the case, the model/simulation needs to be sufficiently flexible or robust to accommodate changing requirements.  Additionally, the model and or simulation needs to accurately address the functionality of the system.  What is the purpose of the system and following that what are the functions that the system needs to do or what functions it must perform to realize the intended purpose.  Therefore, successfully employing and applying the SE process to models/simulation will assist in formulating the model or simulation that assumes the right requirement, or is sufficiently robust to accommodate changing requirements, accurately capture the function that the system is designed to perform, and lastly synthesize the results which should be compared to empirical data, if available, to validate the model such that it can be used to predict the performance of the system and obtain reasonably accurate results. 


1.1.3 Application


One or two paragraphs on where this would be helpful


Life-Cycle Sustainment Analyses


Over two-thirds of the life cycle cost of an acquired system is contained in the cost to operate and support a system.  Given this fact, one way SEs view sustainment is how to lessen the cost of sustainment of an acquired system.  The path that has the greatest impact to reduce the sustainment costs of an acquired system is up front in the acquisition process, during concept exploration or during the preliminary and detailed design phases of an acquisition program.  It is here, in early design, where sustainment costs can be most impacted.  If a design results in a system that has very low “ilities” driving maintainability costs high and time to maintain high, then the other “ilities” to include availability or Ao and reliability tend to be very poor and costly.  A design that keeps in mind how, frequency, who (can the system be sustained at the organizational level or does more costly forms of sustainment such as intermediate or depot level maintenance will be needed.) the system will be maintained/sustained,  SE is all about risk identification and mitigation. A system that has a high cost to sustain and or maintain it poses a risk to the viability of endurance of the system.  SE’s will seek to design and develop a system that takes into account cost, frequency, level of expertise and disposal considerations during the up front, design phase of an acquisition system. One or two paragraph s on how SEs look at sustainment


Markov Analyses


One or two paragraphs on why Markov is useful

A classic way to describe the evolution of a system and its life-cycle is to ascribe its behavior to Markov processes, in which each condition or state of system has a set of predictable probabilities for the condition or state to follow.  This usually formulated as:

    P{Xn+1=j|Xn=i, Xn-1=in-1,…,X0=i0}=P{Xn+1=j|Xn=i}


Where the probability of the next state ( Xn+1) is known if the current state ( Xn) is known. This gives the simulation team a straightforward process of identifying, amalgamating and implementing a set of stochastic processes in their code to generate a series of predictions about future states.  The issue that is not scalable is the issue of how many factors there are in the probabilities under investigation.  In systems engineering the life-cycle sustainment of major DoD systems, the number can become incomprehensibly large. 

In many large systems there is a significant body of information about what state Xn+1 will be if we know state Xn, e.g. we know the impact of ambient temperature change on the internal temperature of a crew saved weapon.  Two issues rather rapidly arise, however: 1) are there some processes that are not Markovian, i.e. are dependent on past states and 2) are the possibilities so numerous, complex, and variable as to make computing any extrema virtually impossible using digital computing techniques, even very massive parallel processing clusters or “the cloud.{


Hidden Markov Analyses\

Not uncommon in defense work, the Hidden Markov also is amenable to computer simulation.  In this case, the states of the process are not directly visible, but the new states produced by the process do become visible in order and the new states can be used to determine previous states.  Given field reports of system states or intelligence reports of unobservable systems, the simulation community can assess varying possible processes that may have produced such observed states and thereby do a better job of estimating both past and futures states of friendly and enemy systems.  Laying aside the possibility of erroneous or intentionally deceptive information, such and analysis is feasible, modulo the impact of too many variables to successfully simulate using current technologies. 

One approach that has been successful in these analyses is the Viterbi algorithm that is widely used in communications systems management and voice recognition.  [6] There is significant conversation in the community about the use of the Viterbi algorithm to analyze Hidden Markov processes in a general way.  [7] This might prove especially useful when modeling “red force” in battlefield simulations/


	Para 2.4 OK DOD requires new fiscal reality – what can Quantum  ComputingQuantum Computing bring to the table? 



One or two paragraphs on how this may be the right model for simulations
NEXT PARAGRAPH Tomorrow


Martingale Analyses

Martingale analyses are also useful in systems engineering and may be employed successfully in simulations of life-cycle sustainment for the analysis of that sustainment or for the better simulation of weapons’ capabilities on the live, virtual or constructive battlefield. Unlike Markov, martingale analyses take very good heed of and are influenced by previously states. The basic formulation for this set of affairs is:

a) E(xn) < µ,       
and
(b)          E(xn+1 | x1,…,xn) = xn 

In the above, the expected state of X is dependent on the previously states, which must be defined in some detail.
 
As before, what is a simple simulation problem on its face, soon spirals out of control as the number of parameters that influence the system grow alarmingly.  This is a well recognized and often discussed problem in simulation: the implementation of reasonable models without swamping available computer resources.  

Clearly the shortcomings of the Markov models with their discounting of the previous trends and impacts of earlier states are addressed by the martingale analyses that acknowledge that which has gone before.  Naturally, in doing so, they multiply the parameters that must be identified, quantified and utilized.  That process alone may seem daunting, but it is the realm of systems engineers. [8]


One or two paragraphs on why this makes better sense


Early Findings



One or two paragraphs on Burns’ dissertation theses



Merging Simulation and Systems engineering

	
	Para 3.1 Quantum & DODAF views.  IE Quantum computing can help the DOD Program Manager navigate through all these views. 

ujOne or two paragraphs on what it would take to better integrate SE and simulation

NEXT PARAGRAPH Tomorrow



Use of High Performance Computing

Mandates for DoD research closely follow the vagaries of scientific innovation and discovery. international events.  The rapidly changing geopolitical environment also imposes a rapidly changing research agenda. [9]. The High Performance Computing (HPC) professionals are in the forefront of these groups being impacted by those changes.  They are tasked with projecting the future of US weapons, systems, tactics and strategies.  Using HPC for battlefield simulation leads to experiments in which warfighters in uniform are staffing the consoles during interactive, HPC-supported simulations.  Experiments to model and simulate the complexities of urban warfare use well-validated entity-level simulations, e.g. Joint Semi-Automated Forces (JSAF) and the Simulation of the Location and Attack of Mobile Enemy Missiles (SLAMEM). These need to be run at a scale and resolution adequate for modeling all the convolutions of urban combat.  

There is a long lineage of entity-level synthetic battlefield codes.  They consist of representations of terrain that are populated with intelligent-agents representing: friendly forces, enemy forces and civilian groups.  Experience has shown that to produce their behaviors in at timely manner, significant compute resources are required [10]. Much of this is true because a major computational load is imposed in the performance of line-of-sight calculations between the entities.  The inherently onerous “n-squared” growth-characteristics of an all-see-all program have been identified previously [11].  If several thousand entities need to interact with each other in an urban setting with vegetation and buildings obscuring the lines of sight, inter-node communications chaos and failure are often observed. This situation has been successfully ameliorated, but only partially so, by the use of an innovative interest-managed communication’s architecture [12].  

Increasingly, DoD simulators required an enhanced Linux clusters of adequate size, power, and configuration to support larger and more sophisticated simulations, especially when there is a requirement for more than 2,000,000 entities within high-resolution insets on a global-scale terrain database.   The cluster has been used occasionally to interact with live exercises, but more often has been engaged interactively with users and experimenters while generating only virtual or constructive simulations. [13] It had to be robust to reliably support hundreds of personnel committed to the experiments and it had to be scalable to easily handle small activities as well as larger global-scale experiments with hundreds of live participants, many distributed trans-continentally, as shown in Figure 1 below.

Creating a standing experimentation environment that can respond immediately to DoD time-critical needs for analysis is one of the major, but difficult to achieve, goals. The operators must operate in a distributed fashion over the Defense Research and Engineering Network (DREN), at a scale and level of resolution that allowed dispersed participants to conduct experimentation on issues of concern to combatant commanders, who have participated in the experiments themselves. This provided the requisite simulation federations, software, and networks, joined into one common computer infrastructure that was supporting experiments. Quantitative and qualitative analysis, flexible plug-and-play standards, and the opportunity for diverse organizations to participate in experiments were all mandated by DoD needs. 

To order to meet these goals, a team from the Information Sciences of the University of Southern California helped design and develop a scalable simulation code that has been shown capable of modeling more than 1,000,000 entities.  This effort is known as the Joint Experimentation on Scalable Parallel Processors (JESPP) project [14]. The dedicated compute power provided additionally allows for the easy identification, collection, and analysis of the voluminous data from these experiments, enabled by the work of Dr. Ke-Thia Yao and his team [15]. 

[image: Joshua-Koa_Glenn-Net]
Figure 1
JFCOM’s Experimentation network: 
MHPCC, SPAWAR, ASC-MSRC,
TEC/IDA and JFCOM

Even using these powerful computers, the JFCOM experimenters were constrained in a number of dimensions, e.g. number of entities, sophistication of behaviors, realism of various environmental phenomenology, etc. While the scalability of the code would have made the use of larger clusters feasible, a more effective, efficient, economical and elegant solution was sought.  The end of the Moore’s Law speed and power improvements decreed that eventually JFCOM would need to seek new ways to deliver their services to increasingly sophisticated users with increasingly complex and geographically diverse conflict environments. One approach is the use of more powerful clusters, especially a GPU-enhanced cluster.

The use of existing DOD simulation codes on advanced Linux clusters operated by JFCOM was the implementation method chosen as being most efficient. This effort supplanted the previous JFCOM J9 DC clusters with a new cluster enhanced with 64-bit CPUs and nVidia 8800 graphics processing units (GPUs).  Further, the authors were able to modify a few legacy codes. As noted above, the initial driver for the FMS use of accelerator-enhanced nodes was principally the faster processing of line-of-sight calculations. Envisioning other acceleration targets is easy: physics-based phenomenology, CFD plume dispersion, computational atmospheric chemistry, data analysis, etc. The computer was given the Joshua, the Hebrew commander.

[image: GPGPU-ClusterJFCOM]

[bookmark: _Toc253135271]Figure 2
Joshua

While great strides were made in the number of entities to be simulated, the research implications of this achievement, albeit expected, were a dramatic reaffirmation of the value of HPCs.  Most notably, on 14 December 2007, the Joint Forces Command Personnel, under the leadership of Rich Williams simulated a full ten million CultureSAF entities on the Baghdad terrain database.  This was accomplished as is visualized in Figure 3 below:

[image: SPP test]

[bookmark: _Ref253057936][bookmark: _Toc253135270]Figure 3
Graph of Entity Count Grow by Time on 14 Dec 07


Introduction of Quantum Computing


Members of the simulation community are often seeking new capabilities to enhance their computational power. The growth of transistor density, and the related capability of traditional digital computing, postulated by Moore's Law [16] is approaching its limits asymptotically. Hence the need to more seriously reevaluate new computing paradigms. One of the most often discussed paths is quantum computing and its first practical incarnation, adiabatic quantum annealing [17]. This section focuses on issues of concern to the test and evaluation application developers. It presents an overview of quantum computing, a review of some early work on a D-Wave quantum annealer at the University of Southern California and a discussion of the applicability of this technology to simulation. It is not a learned treatise on the theoretical and mathematical intricacies of quantum computing nor does it advocate some specific resolution of the many issues that arise with the introduction of any new technology. Instead, the authors rely on decades of experience in high performance computing and DoD simulations to offer aid to the test and evaluation community in assessing the potential utility of this advance. 

According to Gordon Moore himself, the end of Moore's Law is nigh. It is increasingly daunting to continue on the current transistor-based path for increasing the traditional digital computing capability that can be applied to test and evaluation and other national security challenges. The capability growth of individual processors is stagnating and the number of such cores needed is now increasing exponentially in high performance computing systems. Size and power demands now often constrain the computational power that can be brought to bear on defense problems. In this environment, there is a growing interest in alternatives to commercial, off-the-shelf (COTS) technology, which would have seemed inconceivable for most of the last two decades. In many ways, this may be the reemergence of the purpose built systems of earlier decades. New installations include specialized systems such as the Anton at D. E. Shaw Research [18][19] It performs certain biomolecular simulations nearly two orders-of-magnitude faster than the largest general purpose computers. Others are looking beyond CMOS to exploit other physical phenomenon, e.g. quantum computing.

There has sprung up a considerable body of proffesional interest in Quantum Computing beginning with a ground-breaking paper from the Nobel Laureate Richard Feynman in 1982 [20], in which he said “… with a suitable class of quantum machines you could imitate any quantum system, including the physical world.”. The authors are unaware of any such “general purpose” quantum computer that is even nearing operation. However, a more manageable adiabatic quantum annealing device has been conceived, designed, produced, and delivered to the University of Southern California. Figure 4 shows the D-Wave Two, as installed in the USC – Lockheed Martin Quantum Computing Center (QCC) at the Information Sciences Institute (ISI) in Marina del Rey (ISI, 2015)[image: ]

Figure 4
USC QCC D-Wave 2


In recent years, other authors have touted quantum computing’s ability to produce more power, using terms like “magic” to stir the imagination and whet the appetites of the user community. [21] They point out that the capability of quantum computers arises from the different way they encode information. Digital computers represent information with transistor-based switches having a state of 0 or 1, labeled a bit. In contrast, the basic unit of quantum computer operation, the quantum bit or qubit, can exist simultaneously as 0 and 1, with the probability of each being given by a numerical coefficient, a condition physicists call “superposition”. The quantum computer can act on all these possible states simultaneously. 

The authors have witnessed and participated in the development of high performance computing for several decades and have developed a significant body of experience with newly introduced technologies. They were engaged in the very early introduction of parallel computing and aware of its rivalry with sequential computing and with vector computing. They heard the detractors of parallel computing argue the limits of parallelism [22] and the proponents [23] who argued that it could be used more universally. While acknowledging there are many problems that have remained outside of the easily parallelized arena, it is evident that the majority of all large-scale computational problems are now run in parallel. This is due to the application of new techniques to decompose both data and computation in effective ways [24]. Such technology has proven very useful to the simulation community [25] [26] and which may very well have a revolutionary impact as its abilities to resolved currently intractable problems. 

The D-Wave Quantum Annealers have demonstrated acceptable evidence that they are operating as a quantum device, but the high levels of performance gains are yet to be achieved were anticipated.  This may indicate just the issues that always have arrived with any new technology [27], or it may reflect some fatal flaw in the approach. Current work at USC and at Ames seems likely to resolve this issue in the upcoming months.  Nevertheless, it should be remembered that this will not be the general purpose quantum computer envisioned by Feynman, but a quantum annealer, capable of many analytic and optimization analyses of vital interest to the simulation community.

Quantum Computing and Markov/Martingale Analyses 

Given the virtually boundless number of inputs into any analysis of life-cycle sustainment, the simulation of those processes becomes an overwhelming task in short order.  N squared growth in computing requirements quickly mandates some drastic action.  Heretofore a common solution was to substitute a “look-up” table for actual simulation of the physical or behavioral characteristics of the simulated entity.  In some cases this was rational and easily implemented.  In others, a serious problem arose with the questions as to the validity of such a table and the number of factors that would impact on that solution.

As many of these issues involve an optimization function, not a specific physical simulation, simulated annealing becomes a viable alternative.  If annealing is feasible, then Adiabatic Quantum Annealing may hold promise of a truly valid and rapid solution.  The authors assert that all of the analyses proposed here should be amenable to the computational power of the Quantum Annealer.  Should the need arise for pursuing this route, the current D-Wave Annealers are capable of accepting a set of test codes to ascertain if the process can be implemented on the existing hardware. As these machines become larger and more capable, they should  be able to provide the kinds of power to make system engineering life-cycle sustainment simulations possible and enable similar simulation efforts. 
Half a page on how QA can enable these analyses

Potential for further Collaboration



D-Wave Quantum Annealers have extraordinary potential for further collaboration with the DOD acquisition life cycles sustainment and testing communities.  

One or two paragraphs on what this might mean for community

NEXT PARAGRAPH Tomorrow


Analysis


One or two paragraphs on the need to organize

NEXT PARAGRAPH Tomorrow

Mapping a Future Course

NEXT PARAGRAPH Tomorrow

[bookmark: _GoBack]System Engineers would benefit from increased Investment and Research (I&R) for D-Wave Quantum Annealers in the future. These benefits would assist DoD PM’s in  

One or two paragraphs on who and what to engage

Understanding the Problems


SEs strive to understand the problems or pitfalls in the design, development and fielding of acquisition systems. To reduce the risk of pitfalls and mitigate risks in the acquisition of new systems, SE’s draw upon past experiences and lessons learned from previous similar acquisition programs. What were the lessons learned, what were their impact? How can these lessons learned be applied to the acquisition of future systems so the same pitfalls will not be repeated? These lessons learned  become the baseline risks to be considered and generate a risk matrix for the acquisition system. The risk matrix plots the likelihood of a risk occurring versus significance of impact on the system should the risk occur.  SEs weigh this information to help drive decisions where resources will be made available to mitigate these risks. One or two paragraphs looking at pitfalls and risks

Reacting to new Requirements

Previously stated, the robustness of a model/simulation is measured by its flexibility in reacting to new requirements.  One phenomena, if not checked and addressed throughout the acquisition life cycle process is what is known as “Requirements Creep”  While it is understood that new requirements will emerge during the acquisition process of a system as information about the objective and functionality of the system gets further defined resulting from more knowledge about the objective or goal of the system, it is important to keep to a minimum this phenomena of Requirements Creep as it will have, as an examination of previous acquisition programs subject to Requirements Creep, a detrimental and sometimes unrecoverable consequence to a program. The Navy’s DDG-1000 program ended up with 10 new technologies resulting from the identified requirements that the ship had to meet.  Earlier in its design period, there were significantly more technologies identified as requirement creep raised it ugly head.  But, through judicious examination of the core requirements and functions to address the requirements, the growing list was reduced to the 10 needed new technologies.  This action helped to reduce acquisition cost and keep the ship acquisition and budget close to being on par with available resources to build and deliver the ship.  One or two paragraphs considering new extensibilities


Coding Challenges

One or two paragraphs on programmers’ problems 
Dan -Is this paragraph needed??? 

Conclusions

One or two paragraphs on reiterating the theses


Uses of SEf Systems engineering
	 
SE is extensively employed in the commercial sector as well as the defense industry. As stated previously, a key role of SE is to reduce the risk of designing, developing, testing, certifying and employing systems.  Major Program Managers in the Acquisition Community of the defense industry, resulting from what was previously known as a Missions Need Statement (MNS) conduct Analysis of Alternatives (AoA’s) to a address a specific military need (e.g., requirement) and determine the solution space ranging from the employment of existing equipment, software, policy to developing a new system.  The key tenants of SE which are 1) Requirements, 2) Functional Analysis, and 3) Synthesis are all employed in the acquisition process to identify, reduce and mitigate risks involved with the acquisition of a solution set to address specific military needs and requirements from the beginning of the process, i.e., concept definition through fielding and even disposal of the system; a “cradle to grave” process.
 

Benefits of Parameterization

One benefit of these sorts of analyses is the impact of having to seriously reconsider which parameters are most important and which are merely distractions.  Especially in their early work with parallel computers at Caltech, the authors noted that having to do a disciplined reassessment of the parameters and functions on the topic being simulated was often very illuminating, both in terms of the computational approach, but also in terms of the insights of the user into what was really critical in their systems. 

In the instant case, the multitude of parameters involved in Markov, Hidden Markov and martingale analyses will likely have a salutary impact on the simulation community and on its user clients.  

Para 5.2  Benefits of Parameterization – Can Quantum Computers help the Program MGR?  The definition of insanity is repeating things over and over again using the current PM tools. These tools have enabled failures such as FIA, LCS and FCS.  I’m driving to Monterey this afternoon and working on the article.  MTF.

One or two paragraphs on why quantification is good


Investment Required


Just as the National Ignition Facility is of enormous consequence to the general physics community for the increased scientific benefits that it will return on the investments made (Cost $2B in 2016 dollars – Cite the source). The potential for further collaboration is enormous for  M&S community and the DoD Acquisition community with Quantum Annealers is also required to yield the benefits to future DOD acquisition programs. The N-Squared inputs to a Quantum Annealer will help provide the system engineers those trigger points that will allow the PM to keep the acquisition program on track. 

One or two paragraphs on cost benefit analysis of idea
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Generic Acquisition Process (Pre-Tailoring)
Acquisition Decision Points and Phases

This chart illustrates the sequence of events in a generic program, which could be a Defense program or, except for the unique DoD terminology , a commercial product.
DoD Instruction 5000.02 milestones, other decisions, phases and major phase activities are shown in relation to the generic sequence of events.

The decision that a new product is

L needed and that activities to analyze
Need Identification alternative solutions will occur.

(DoD: Materiel Development
Decision)

/\

Solution Analysis

DoD: Materiel Solution Analysis Phase

* Conduct analysis and other activities needed to choose the concept for the product that will be
acquired.

* Begin translating validated capability gaps into system-specific requirements including the Key
Performance Parameters (KPPs), Key System Attributes (KSAs).

* Conduct planning to support a decision on the acquisition strategy for the product.

* Analysis of Alternative (AoA) solutions, key trades between cost and performance, affordability
analysis, risk analysis, and planning for risk mitigation are key activities in this phase.

* Component Acquisition Executive selects a Program Manager and establishes a program office to
plan the acquisition program with emphasis on the next phase.

Risk Reduction Decision
(DoD: Milestone A)

product or design concepts, and to commit

The generic milestones and decision points illustrated on this chart are standard for DoD; however, Milestone Decision
Authorities (MDAs) have full latitude to tailor programs in the most effective and efficient structure as much as needed to
accommodate the characteristics of the product being acquired, and to the totality of circumstances associated with the
program including operational urgency and risk factors.

* MDAs will tailor program strategies and oversight, including program information, acquisition phase content, the
timing and scope of decision reviews and decision levels, based on the specifics of the product being acquired,
including complexity, risk factors, and required timelines to satisfy validated capability requirements.

* When there is a strong threat-based or operationally driven need to field a capability solution in the shortest time,
MDAs are authorized to implement streamlined procedures designed to accelerate acquisition system
An investment decision to pursue specific responsiveness. Statutory requirements will be complied with, unless waived in accordance with relevant provisions.

Tailoring of Milestones, Decision Points, and Phases

resources required to mature technology and/or
reduce risks that must be mitigated prior to
decision committing the resources needed for
development leading to production and fielding

Technology Maturation and
Risk Reduction

DoD: Technology Maturation and Risk Reduction Phase

* Includes a mix of activities intended to reduce specific risks associated with the

product to be developed.

* Includes additional design trades and requirements trades necessary to ensure an
affordable product and executable development and production programs.

* Normally includes competitive sources conducting technology maturation and risk
reduction activities and preliminary design activities up to and including
Preliminary Design Review prior to source selection for the EMD phase.

Development
Decisions

Legend

A= Decision Point

CDD = Capability Development Document

RFP = Request for Proposal

This chart illustrates the sequence of decision events in a generic program.
It is not intended to reflect the time dedicated to associated phase activity.

—<

The point at which major cost and performance trades
have been completed and enough risk reduction has been
completed to support a decision to commit to the set of

requirements that will be used for preliminary design Development RFP Release Decision
activities, development, and production (subject to . o . L . ) ;
reconsideration and refinement as knowledge increases). The development contract award is the critical decision point in an acquisition program because it commits the

/—Requirements Decision Point
(DoD: CDD Validation)

organization’s resources to a specific product, budget profile, choice of suppliers, contract terms, schedule, and
sequence of events leading to production and fielding. In practice however, almost all of these decisions have to be

The point at which planning for development
is complete and a decision can be made to
release an RFP for development (and possibly

Development RFP initial production) to industry.

made prior to the release of the RFP to industry in order to inform the bidders’ proposals.

For DoD, the RFP release decision point is the point at which plans for the program must be most carefully
reviewed to ensure all risks are understood and under control, the program plan is sound, and that the program

Release Decision

will be affordable and executable.

The decision that commits resources (authorizes
proceeding to award of the contract(s)) needed

to conduct development leading to production

and fielding of the product.

The Development RFP Release Decision is described by the USD(AT&L) as, “the most important single decision
point in the entire life cycle because the release of the Engineering and Manufacturing Development RFP sets in
motion everything that follows in a products life cycle.”

Development Decision
(DoD: Milestone B)

VAN

N~ Development

DoD: Engineering and Manufacturing Development Phase

Complete all hardware and software detailed design.
* Retire any open risks.

* Build and test prototypes or first articles to verify compliance with capability requirements.

* Prepare for production or deployment.

* Successful completion of adequate developmental testing to support entering Low-Rate

Initial Production or Limited deployment.

i

nitial Production Decision difficult and expensive to reverse.
(DoD: Milestone C)

The production decision, usually based on
developmental test results, commits the
resources (i.e., authorizes proceeding to award
the contract(s)) required to enter production
and begin fielding of the product. The
commitment to enter production is very

Low-Rate Initial Production (LRIP) or Limited
Deployment and Operational Test

Production <
Decisions

DoD: Production and Deployment Phase

* LRIP establishes the initial production base for the system, provides operational test
articles, provides an efficient ramp up to full rate production, and maintains
continuity in production pending completion of operational test and evaluation.

* LRIP equivalent for software systems is typically limited deployment or limited

fielding. The decision, following completion of
* While this portion of the phase should be of limited duration so that efficient operational testing of representative initial
production rates and/or full fielding can be accomplished as soon and as economically production products, to scale-up production

as possible, it should be of sufficient duration to permit identification and resolution
of any significant deficiencies prior to full rate production.

Full-Rate Production/Full Deployment
(DoD: Full-Rate Production/Full Deployment Decision)

/\

and/or fielding.

DoD: Production and Deployment Phase, continued... =~ 777U
* Remaining production or deployment of the product is completed, leading to Full Sustainment DiSpOSBl
Operational Capability or Full Deployment. e
* Except as specifically approved by the MDA, critical deficiencies identified in DoD: Operatlons and SuPport Phase
testing will be resolved prior to proceeding beyond LRIP or Limited Deployment. * The product support strategy is executed to satisfy materiel readiness and
operational support performance requirements, and sustain the system over
its life cycle.

* At the end of its useful life, system is demilitarized and disposed of in
accordance with all legal and regulatory requirements and policy relating to
safety (including explosives safety), security, and the environment.
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Need Identification 

(DoD: Materiel Development 

Decision) 

Solution Analysis 

Risk Reduction Decision 

(DoD: Milestone A) 

Requirements Decision Point 

(DoD: CDD Validation) 

Development RFP 

Release Decision  

DoD: Materiel Solution Analysis Phase 

•Conduct analysis and other activities needed to choose the concept for the product that will be 

acquired. 

•Begin translating validated capability gaps into system-specific requirements including the Key 

Performance Parameters (KPPs), Key System Attributes (KSAs). 

•Conduct planning to support a decision on the acquisition strategy for the product. 

•Analysis of Alternative (AoA) solutions, key trades between cost and performance, affordability 

analysis, risk analysis, and planning for risk mitigation are key activities in this phase. 

•Component Acquisition Executive selects a Program Manager and establishes a program office to 

plan the acquisition program with emphasis on the next phase. 

An investment decision to pursue specific 

product or design concepts, and to commit 

resources required to mature technology and/or 

reduce risks that must be mitigated prior to 

decision committing the resources needed for 

development leading to production and fielding  

The decision that a new product is 

needed and that activities to analyze 

alternative solutions will occur. 

Development Decision 

(DoD: Milestone B) 

The decision that commits resources (authorizes 

proceeding to award of the contract(s)) needed 

to conduct development leading to production 

and fielding of the product.  

DoD: Engineering and Manufacturing Development Phase 

•Complete all hardware and software detailed design. 

•Retire any open risks. 

•Build and test prototypes or first articles to verify compliance with capability requirements. 

•Prepare for production or deployment. 

•Successful completion of adequate developmental testing to support entering Low-Rate 

Initial Production or Limited deployment. 

Development 

Decisions 

Development RFP Release Decision 

The development contract award is the critical decision point in an acquisition program because it commits the 

organization’s resources to a specific product, budget profile, choice of suppliers, contract terms, schedule, and 

sequence of events leading to production and fielding. In practice however, almost all of these decisions have to be 

made prior to the release of the RFP to industry in order to inform the bidders’ proposals.  

For DoD, the RFP release decision point is the point at which plans for the program must be most carefully 

reviewed to ensure all risks are understood and under control, the program plan is sound, and that the program 

will be affordable and executable.  

The Development RFP Release Decision is described by the USD(AT&L) as, “the most important single decision 

point in the entire life cycle because the release of the Engineering and Manufacturing Development RFP sets in 

motion everything that follows in a products life cycle.” 

The point at which major cost and performance trades 

have been completed and enough risk reduction has been 

completed to support a decision to commit to the set of 

requirements that will be used for preliminary design 

activities, development, and production (subject to 

reconsideration and refinement as knowledge increases). 

The point at which planning for development 

is complete and a decision can be made to 

release an RFP for development (and possibly 

initial production) to industry. 

Initial Production  Decision 

(DoD: Milestone C) 

The production decision, usually based on 

developmental test results, commits the 

resources (i.e., authorizes proceeding to award 

the contract(s)) required to enter production 

and begin fielding of the product. The 

commitment to enter production is very 

difficult and expensive to reverse. 

Full-Rate Production/Full Deployment 

(DoD: Full-Rate Production/Full Deployment Decision) 

DoD:  Technology Maturation and Risk Reduction Phase 

•Includes a mix of activities intended to reduce specific risks associated with the 

product to be developed. 

•Includes additional design trades and requirements trades necessary to ensure an 

affordable product and executable development and production programs. 

•Normally includes competitive sources conducting technology maturation and risk 

reduction activities and preliminary design activities up to and including 

Preliminary Design Review prior to source selection for the EMD phase. 

DoD: Production and Deployment Phase 

•LRIP establishes the initial production base for the system, provides operational test 

articles, provides an efficient ramp up to full rate production, and maintains 

continuity in production pending completion of operational test and evaluation. 

•LRIP equivalent  for software systems is typically limited deployment or limited 

fielding. 

•While this portion of the phase should be of limited duration so that efficient 

production rates and/or full fielding can be accomplished as soon and as economically 

as possible, it should be of sufficient duration to permit identification and resolution 

of any significant deficiencies prior to full rate production. 

 

Production 

Decisions 

The decision, following completion of 

operational testing of representative initial 

production products, to scale-up production 

and/or fielding. 

Legend 

         = Decision Point 

CDD = Capability Development Document 

RFP  = Request for Proposal 

This chart illustrates the sequence of decision events in a generic program. 

It is not intended to reflect the time dedicated to associated phase activity. 

Tailoring of Milestones, Decision Points, and Phases 

The generic milestones and decision points illustrated on this chart are standard for DoD; however, Milestone Decision 

Authorities (MDAs) have full latitude to tailor programs in the most effective and efficient structure as much as needed  to 

accommodate the characteristics of the product being acquired, and to the totality of circumstances associated with the 

program including operational urgency and risk factors.  

•

MDAs will tailor program strategies and oversight, including program information, acquisition phase content, the 

timing and scope of decision reviews and decision levels, based on the specifics of the product being acquired, 

including complexity, risk factors, and required timelines to satisfy validated capability requirements. 

•

When there is a strong threat-based or operationally driven need to field a capability solution in the shortest time, 

MDAs are authorized to implement streamlined procedures designed to accelerate acquisition system 

responsiveness. Statutory requirements will be complied with, unless waived in accordance with relevant provisions. 

DoD: Production and Deployment Phase, continued… 

•Remaining production or deployment of the product is completed, leading to Full 

Operational Capability or Full Deployment.   

•Except as specifically approved by the MDA, critical deficiencies identified in 

testing will be resolved prior to proceeding beyond LRIP or Limited Deployment. 

DoD: Operations and Support Phase 

•The product support strategy is executed to satisfy materiel readiness and 

operational support performance requirements, and sustain the system over 

its life cycle.  

•At the end of its useful life, system is demilitarized and disposed of in 

accordance with all legal and regulatory requirements and policy relating to 

safety (including explosives safety), security, and the environment.  

Solution Analysis 

Generic Acquisition Process (Pre-Tailoring) 

Acquisition Decision Points and Phases 

This chart illustrates the sequence of events in a generic program, which could be a Defense program or, except for the unique DoD terminology , a commercial product.  

DoD Instruction 5000.02  milestones, other decisions, phases and major phase activities are shown in relation to the generic sequence of events. 

Low-Rate Initial Production (LRIP) or Limited 

Deployment and Operational Test 

Disposal 

Sustainment 

Development 

Technology Maturation and  

Risk Reduction 

Production, Deployment and Sustainment 
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